This EDS file is made for the FCAN-01 CANopen adapter module,
which is a module for connecting ABB Drives to the CANopen network.

The EDS files are named in the format FCAN-01_[Module FW revision]_[Drive]_[Drive FW revision]_[EDS file revision].EDS
For example, the EDS file for FCAN-01 version 102B and the ACS355 Drive with FW version 5.02C
is named FCAN-01_102B_ACS355_5.02C_Extended_Vector_V1.8.EDS. Note, for some drives it is necessary to have 
different files for Scalar and Vector motor control modes. If this is the case, the supported motor control mode is
displayed in the file name.

The EDS files are generated for a specific drive/module version configuration. However, they are
also usable with other drive and module firmware versions. ABB does not supply EDS files for all
firmware versions.